--- a/arch/mips/ath79/mach-pb44.c
+++ b/arch/mips/ath79/mach-pb44.c
@@ -8,23 +8,48 @@
  *  by the Free Software Foundation.
  */
 
+#include <linux/delay.h>
 #include <linux/init.h>
 #include <linux/platform_device.h>
 #include <linux/i2c.h>
 #include <linux/i2c-gpio.h>
 #include <linux/i2c/pcf857x.h>
+#include <linux/i2c/pcf857x.h>
+#include <linux/spi/flash.h>
+#include <linux/spi/vsc7385.h>
 
-#include "machtypes.h"
+#include <asm/mach-ath79/ar71xx_regs.h>
+#include <asm/mach-ath79/ath79.h>
+
+#include "dev-eth.h"
 #include "dev-gpio-buttons.h"
 #include "dev-leds-gpio.h"
 #include "dev-spi.h"
 #include "dev-usb.h"
+#include "machtypes.h"
 #include "pci.h"
 
 #define PB44_GPIO_I2C_SCL	0
 #define PB44_GPIO_I2C_SDA	1
 
+#define PB44_PCF8757_VSC7395_CS	0
+#define PB44_PCF8757_STEREO_CS	1
+#define PB44_PCF8757_SLIC_CS0	2
+#define PB44_PCF8757_SLIC_TEST	3
+#define PB44_PCF8757_SLIC_INT0	4
+#define PB44_PCF8757_SLIC_INT1	5
+#define PB44_PCF8757_SW_RESET	6
+#define PB44_PCF8757_SW_JUMP	8
+#define PB44_PCF8757_LED_JUMP1	9
+#define PB44_PCF8757_LED_JUMP2	10
+#define PB44_PCF8757_TP24	11
+#define PB44_PCF8757_TP25	12
+#define PB44_PCF8757_TP26	13
+#define PB44_PCF8757_TP27	14
+#define PB44_PCF8757_TP28	15
+
 #define PB44_GPIO_EXP_BASE	16
+#define PB44_GPIO_VSC7395_CS	(PB44_GPIO_EXP_BASE + PB44_PCF8757_VSC7395_CS)
 #define PB44_GPIO_SW_RESET	(PB44_GPIO_EXP_BASE + 6)
 #define PB44_GPIO_SW_JUMP	(PB44_GPIO_EXP_BASE + 8)
 #define PB44_GPIO_LED_JUMP1	(PB44_GPIO_EXP_BASE + 9)
@@ -92,21 +117,66 @@ static struct ath79_spi_controller_data
 	.cs_line = 0,
 };
 
+static struct ath79_spi_controller_data pb44_spi1_data = {
+	.cs_type = ATH79_SPI_CS_TYPE_GPIO,
+	.cs_line = PB44_GPIO_VSC7395_CS,
+};
+
+static void pb44_vsc7395_reset(void)
+{
+	ath79_device_reset_set(AR71XX_RESET_GE1_PHY);
+	udelay(10);
+	ath79_device_reset_clear(AR71XX_RESET_GE1_PHY);
+	mdelay(50);
+}
+
+static struct vsc7385_platform_data pb44_vsc7395_data = {
+	.reset		= pb44_vsc7395_reset,
+	.ucode_name	= "vsc7395_ucode_pb44.bin",
+	.mac_cfg = {
+		.tx_ipg		= 6,
+		.bit2		= 1,
+		.clk_sel	= 0,
+	},
+};
+
+static const char *pb44_part_probes[] = {
+	"RedBoot",
+	NULL,
+};
+
+static struct flash_platform_data pb44_flash_data = {
+	.part_probes	= pb44_part_probes,
+};
+
 static struct spi_board_info pb44_spi_info[] = {
 	{
 		.bus_num	= 0,
 		.chip_select	= 0,
 		.max_speed_hz	= 25000000,
 		.modalias	= "m25p64",
+		.platform_data	= &pb44_flash_data,
 		.controller_data = &pb44_spi0_data,
 	},
+	{
+		.bus_num	= 0,
+		.chip_select	= 1,
+		.max_speed_hz	= 25000000,
+		.modalias	= "spi-vsc7385",
+		.platform_data	= &pb44_vsc7395_data,
+		.controller_data = &pb44_spi1_data,
+	}
 };
 
 static struct ath79_spi_platform_data pb44_spi_data = {
 	.bus_num		= 0,
-	.num_chipselect		= 1,
+	.num_chipselect		= 2,
 };
 
+#define PB44_WAN_PHYMASK	BIT(0)
+#define PB44_LAN_PHYMASK	0
+#define PB44_MDIO_PHYMASK	(PB44_LAN_PHYMASK | PB44_WAN_PHYMASK)
+
 static void __init pb44_init(void)
 {
 	i2c_register_board_info(0, pb44_i2c_board_info,
@@ -122,6 +192,22 @@ static void __init pb44_init(void)
 			   ARRAY_SIZE(pb44_spi_info));
 	ath79_register_usb();
 	ath79_register_pci();
+
+	ath79_register_mdio(0, ~PB44_MDIO_PHYMASK);
+
+	ath79_init_mac(ath79_eth0_data.mac_addr, ath79_mac_base, 0);
+	ath79_eth0_data.phy_if_mode = PHY_INTERFACE_MODE_RGMII;
+	ath79_eth0_data.phy_mask = PB44_WAN_PHYMASK;
+
+	ath79_register_eth(0);
+
+	ath79_init_mac(ath79_eth1_data.mac_addr, ath79_mac_base, 1);
+	ath79_eth1_data.phy_if_mode = PHY_INTERFACE_MODE_RGMII;
+	ath79_eth1_data.speed = SPEED_1000;
+	ath79_eth1_data.duplex = DUPLEX_FULL;
+	ath79_eth1_pll_data.pll_1000 = 0x110000;
+
+	ath79_register_eth(1);
 }
 
 MIPS_MACHINE(ATH79_MACH_PB44, "PB44", "Atheros PB44 reference board",
--- a/arch/mips/ath79/Kconfig
+++ b/arch/mips/ath79/Kconfig
@@ -58,6 +58,7 @@ config ATH79_MACH_DB120
 config ATH79_MACH_PB44
 	bool "Atheros PB44 reference board"
 	select SOC_AR71XX
+	select ATH79_DEV_ETH
 	select ATH79_DEV_GPIO_BUTTONS
 	select ATH79_DEV_LEDS_GPIO
 	select ATH79_DEV_SPI
