From 6c223da976a9225ba9fae8d6f891a8fffaae6092 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <zajec5@gmail.com>
Date: Fri, 5 Dec 2014 17:38:40 +0100
Subject: [PATCH] ARM: BCM5301X: Enable ChipCommon UART (serial console)
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Signed-off-by: Rafał Miłecki <zajec5@gmail.com>
---
 arch/arm/boot/dts/bcm4708-buffalo-wzr-1750dhp.dts  | 10 ++++++++++
 arch/arm/boot/dts/bcm4708-netgear-r6300-v2.dts     | 10 ++++++++++
 arch/arm/boot/dts/bcm47081-asus-rt-n18u.dts        | 10 ++++++++++
 arch/arm/boot/dts/bcm47081-buffalo-wzr-600dhp2.dts | 10 ++++++++++
 4 files changed, 40 insertions(+)

--- a/arch/arm/boot/dts/bcm4708-netgear-r6300-v2.dts
+++ b/arch/arm/boot/dts/bcm4708-netgear-r6300-v2.dts
@@ -83,3 +83,7 @@
 		};
 	};
 };
+
+&uart0 {
+	status = "okay";
+};
--- a/arch/arm/boot/dts/bcm47081-asus-rt-n18u.dts
+++ b/arch/arm/boot/dts/bcm47081-asus-rt-n18u.dts
@@ -77,3 +77,7 @@
 		};
 	};
 };
+
+&uart0 {
+	status = "okay";
+};
--- a/arch/arm/boot/dts/bcm47081-buffalo-wzr-900dhp.dts
+++ b/arch/arm/boot/dts/bcm47081-buffalo-wzr-900dhp.dts
@@ -37,3 +37,7 @@
 		};
 	};
 };
+
+&uart0 {
+	status = "okay";
+};
--- a/arch/arm/boot/dts/bcm4709-asus-rt-ac87u.dts
+++ b/arch/arm/boot/dts/bcm4709-asus-rt-ac87u.dts
@@ -65,3 +65,8 @@
 		};
 	};
 };
+
+&uart0 {
+	status = "okay";
+	clock-frequency = <125000000>;
+};
--- a/arch/arm/boot/dts/bcm4709-netgear-r8000.dts
+++ b/arch/arm/boot/dts/bcm4709-netgear-r8000.dts
@@ -108,6 +108,11 @@
 	};
 };
 
+&uart0 {
+	status = "okay";
+	clock-frequency = <125000000>;
+};
+
 &usb2 {
 	vcc-gpio = <&chipcommon 0 GPIO_ACTIVE_HIGH>;
 };
--- a/arch/arm/boot/dts/bcm4708-asus-rt-ac56u.dts
+++ b/arch/arm/boot/dts/bcm4708-asus-rt-ac56u.dts
@@ -96,3 +96,7 @@
 		};
 	};
 };
+
+&uart0 {
+	status = "okay";
+};
--- a/arch/arm/boot/dts/bcm4708-asus-rt-ac68u.dts
+++ b/arch/arm/boot/dts/bcm4708-asus-rt-ac68u.dts
@@ -83,3 +83,7 @@
 		};
 	};
 };
+
+&uart0 {
+	status = "okay";
+};
--- a/arch/arm/boot/dts/bcm4709-buffalo-wxr-1900dhp.dts
+++ b/arch/arm/boot/dts/bcm4709-buffalo-wxr-1900dhp.dts
@@ -145,6 +145,10 @@
 	};
 };
 
+&uart0 {
+	status = "okay";
+	clock-frequency = <125000000>;
+};
 
 &usb2 {
 	vcc-gpio = <&chipcommon 13 GPIO_ACTIVE_HIGH>;
--- a/arch/arm/boot/dts/bcm4709-netgear-r7000.dts
+++ b/arch/arm/boot/dts/bcm4709-netgear-r7000.dts
@@ -104,4 +104,5 @@
 
 &uart0 {
 	status = "okay";
+	clock-frequency = <125000000>;
 };
