#!/bin/sh
#
# Copyright (C) 2014 OpenWrt.org
#

. /lib/functions/uci-defaults.sh
. /lib/mvebu.sh

board=$(mvebu_board_name)

case "$board" in
armada-385-linksys-caiman)
	ucidef_set_led_netdev "wan" "WAN" "pca963x:caiman:white:wan" "eth0"
	ucidef_set_led_usbdev "usb2" "USB2" "pca963x:caiman:white:usb2" "1-1"
	ucidef_set_led_usbdev "usb3" "USB3" "pca963x:caiman:white:usb3_1" "2-1"
	;;
armada-385-linksys-cobra)
	ucidef_set_led_netdev "wan" "WAN" "pca963x:cobra:white:wan" "eth0"
	ucidef_set_led_usbdev "usb2" "USB2" "pca963x:cobra:white:usb2" "1-1"
	ucidef_set_led_usbdev "usb3" "USB3" "pca963x:cobra:white:usb3_1" "2-1"
	;;
armada-385-linksys-rango)
	ucidef_set_led_netdev "wan" "WAN" "pca963x:rango:white:wan" "eth0"
	ucidef_set_led_usbdev "usb2" "USB2" "pca963x:rango:white:usb2" "1-1"
	ucidef_set_led_usbdev "usb3" "USB3" "pca963x:rango:white:usb3_1" "2-1"
	;;
armada-385-linksys-shelby)
	ucidef_set_led_netdev "wan" "WAN" "pca963x:shelby:white:wan" "eth0"
	ucidef_set_led_usbdev "usb2" "USB2" "pca963x:shelby:white:usb2" "1-1"
	ucidef_set_led_usbdev "usb3" "USB3" "pca963x:shelby:white:usb3_1" "2-1"
	;;
armada-xp-linksys-mamba)
	ucidef_set_led_netdev "wan" "WAN" "mamba:white:wan" "eth1"
	ucidef_set_led_usbdev "usb2" "USB2" "mamba:white:usb2" "1-1"
	ucidef_set_led_usbdev "usb3" "USB3" "mamba:white:usb3_1" "2-2"
	;;

esac

ucidef_commit_leds

exit 0
