From 547c653b64022618250ca9c7c30151927509ae98 Mon Sep 17 00:00:00 2001
From: Arnaud Ebalard <arno@natisbad.org>
Date: Sat, 22 Nov 2014 00:46:39 +0100
Subject: arm: mvebu: define and use common Armada XP SPI pinctrl setting

This patch defines common Armada XP pinctrl settings in armada-xp.dtsi
for the supported SPI interface (MPP36-39) and use it as default
for Armada XP spi interface. That being done, it removes the now
redundant definitions in armada-xp-axpwifiap.dts.

Note: this patch has the potential to break out-of-tree users w/o
specific pinctrl settings for their spi interfaces if the default
above does not match their config (i.e. if they do not use CS0).

Acked-by: Andrew Lunn <andrew@lunn.ch>
Signed-off-by: Arnaud Ebalard <arno@natisbad.org>
Link: https://lkml.kernel.org/r/d404b7abd80ee5a0fd8e8d3586d33cd37740d589.1416613429.git.arno@natisbad.org
Signed-off-by: Jason Cooper <jason@lakedaemon.net>

--- a/arch/arm/boot/dts/armada-xp-axpwifiap.dts
+++ b/arch/arm/boot/dts/armada-xp-axpwifiap.dts
@@ -100,8 +100,6 @@
 
 			spi0: spi@10600 {
 				status = "okay";
-				pinctrl-0 = <&pmx_spi>;
-				pinctrl-names = "default";
 
 				spi-flash@0 {
 					#address-cells = <1>;
@@ -138,11 +136,6 @@
 		marvell,function = "gpio";
 	};
 
-	pmx_spi: pmx-spi {
-		marvell,pins = "mpp36", "mpp37", "mpp38", "mpp39";
-		marvell,function = "spi";
-	};
-
 	pmx_phy_int: pmx-phy-int {
 		marvell,pins = "mpp32";
 		marvell,function = "gpio";
--- a/arch/arm/boot/dts/armada-xp.dtsi
+++ b/arch/arm/boot/dts/armada-xp.dtsi
@@ -43,6 +43,11 @@
 				wt-override;
 			};
 
+			spi0: spi@10600 {
+				pinctrl-0 = <&spi0_pins>;
+				pinctrl-names = "default";
+			};
+
 			i2c0: i2c@11000 {
 				compatible = "marvell,mv78230-i2c", "marvell,mv64xxx-i2c";
 				reg = <0x11000 0x100>;
@@ -248,6 +253,12 @@
 		marvell,function = "sd0";
 	};
 
+	spi0_pins: spi0-pins {
+		marvell,pins = "mpp36", "mpp37",
+			       "mpp38", "mpp39";
+		marvell,function = "spi";
+	};
+
 	uart2_pins: uart2-pins {
 		marvell,pins = "mpp42", "mpp43";
 		marvell,function = "uart2";
