From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <zajec5@gmail.com>
Date: Fri, 17 Jun 2016 12:48:44 +0200
Subject: [PATCH] brcmfmac: use const char * for interface name in brcmf_add_if
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

This function can work just fine with const pointer, it only calls
alloc_netdev which take const as well. Moreover it makes this function
more flexible as some cfg80211 callback may provide const char * as
well, e.g. add_virtual_intf. This will be needed for more advanced
interface management.

Signed-off-by: RafaÅ MiÅecki <zajec5@gmail.com>
Signed-off-by: Kalle Valo <kvalo@codeaurora.org>
---

--- a/drivers/net/wireless/broadcom/brcm80211/brcmfmac/core.c
+++ b/drivers/net/wireless/broadcom/brcm80211/brcmfmac/core.c
@@ -638,7 +638,7 @@ fail:
 }
 
 struct brcmf_if *brcmf_add_if(struct brcmf_pub *drvr, s32 bsscfgidx, s32 ifidx,
-			      bool is_p2pdev, char *name, u8 *mac_addr)
+			      bool is_p2pdev, const char *name, u8 *mac_addr)
 {
 	struct brcmf_if *ifp;
 	struct net_device *ndev;
--- a/drivers/net/wireless/broadcom/brcm80211/brcmfmac/core.h
+++ b/drivers/net/wireless/broadcom/brcm80211/brcmfmac/core.h
@@ -215,7 +215,7 @@ char *brcmf_ifname(struct brcmf_if *ifp)
 struct brcmf_if *brcmf_get_ifp(struct brcmf_pub *drvr, int ifidx);
 int brcmf_net_attach(struct brcmf_if *ifp, bool rtnl_locked);
 struct brcmf_if *brcmf_add_if(struct brcmf_pub *drvr, s32 bsscfgidx, s32 ifidx,
-			      bool is_p2pdev, char *name, u8 *mac_addr);
+			      bool is_p2pdev, const char *name, u8 *mac_addr);
 void brcmf_remove_interface(struct brcmf_if *ifp, bool rtnl_locked);
 void brcmf_txflowblock_if(struct brcmf_if *ifp,
 			  enum brcmf_netif_stop_reason reason, bool state);
