From 981de3c2f27af27fa4c5c952d122b35ee573ab7a Mon Sep 17 00:00:00 2001
From: Dan Haab <dhaab@luxul.com>
Date: Wed, 22 Apr 2015 13:58:33 -0600
Subject: [PATCH] MIPS: BCM47XX: Support Luxul XWR-1750 board
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Signed-off-by: Dan Haab <dhaab@luxul.com>
Acked-by: Rafał Miłecki <zajec5@gmail.com>
Cc: linux-mips@linux-mips.org
Cc: Hauke Mehrtens <hauke@hauke-m.de>
Cc: Dan Haab <dhaab@luxul.com>
Patchwork: https://patchwork.linux-mips.org/patch/9831/
Signed-off-by: Ralf Baechle <ralf@linux-mips.org>
---
 arch/mips/bcm47xx/board.c                          |  1 +
 arch/mips/bcm47xx/buttons.c                        | 11 +++++++++++
 arch/mips/bcm47xx/leds.c                           | 14 ++++++++++++++
 arch/mips/include/asm/mach-bcm47xx/bcm47xx_board.h |  2 ++
 4 files changed, 28 insertions(+)

--- a/arch/mips/bcm47xx/board.c
+++ b/arch/mips/bcm47xx/board.c
@@ -149,6 +149,7 @@ struct bcm47xx_board_type_list2 bcm47xx_
 /* board_id */
 static const
 struct bcm47xx_board_type_list1 bcm47xx_board_list_board_id[] __initconst = {
+	{{BCM47XX_BOARD_LUXUL_XWR_1750_V1, "Luxul XWR-1750 V1"}, "luxul_xwr1750_v1"},
 	{{BCM47XX_BOARD_NETGEAR_WGR614V8, "Netgear WGR614 V8"}, "U12H072T00_NETGEAR"},
 	{{BCM47XX_BOARD_NETGEAR_WGR614V9, "Netgear WGR614 V9"}, "U12H094T00_NETGEAR"},
 	{{BCM47XX_BOARD_NETGEAR_WGR614_V10, "Netgear WGR614 V10"}, "U12H139T01_NETGEAR"},
--- a/arch/mips/bcm47xx/buttons.c
+++ b/arch/mips/bcm47xx/buttons.c
@@ -299,6 +299,13 @@ bcm47xx_buttons_linksys_wrtsl54gs[] __in
 	BCM47XX_GPIO_KEY(6, KEY_RESTART),
 };
 
+/* Luxul */
+
+static const struct gpio_keys_button
+bcm47xx_buttons_luxul_xwr_1750_v1[] = {
+	BCM47XX_GPIO_KEY(14, BTN_TASK),
+};
+
 /* Microsoft */
 
 static const struct gpio_keys_button
@@ -555,6 +562,10 @@ int __init bcm47xx_buttons_register(void
 		err = bcm47xx_copy_bdata(bcm47xx_buttons_linksys_wrtsl54gs);
 		break;
 
+	case BCM47XX_BOARD_LUXUL_XWR_1750_V1:
+		err = bcm47xx_copy_bdata(bcm47xx_buttons_luxul_xwr_1750_v1);
+		break;
+
 	case BCM47XX_BOARD_MICROSOFT_MN700:
 		err = bcm47xx_copy_bdata(bcm47xx_buttons_microsoft_nm700);
 		break;
--- a/arch/mips/bcm47xx/leds.c
+++ b/arch/mips/bcm47xx/leds.c
@@ -370,6 +370,16 @@ bcm47xx_leds_linksys_wrtsl54gs[] __initc
 	BCM47XX_GPIO_LED(7, "orange", "wps", 1, LEDS_GPIO_DEFSTATE_OFF),
 };
 
+/* Luxul */
+
+static const struct gpio_led
+bcm47xx_leds_luxul_xwr_1750_v1[] __initconst = {
+	BCM47XX_GPIO_LED(5, "green", "5ghz", 0, LEDS_GPIO_DEFSTATE_OFF),
+	BCM47XX_GPIO_LED(12, "green", "usb", 0, LEDS_GPIO_DEFSTATE_OFF),
+	BCM47XX_GPIO_LED_TRIGGER(13, "green", "status", 0, "timer"),
+	BCM47XX_GPIO_LED(15, "green", "wps", 0, LEDS_GPIO_DEFSTATE_OFF),
+};
+
 /* Microsoft */
 
 static const struct gpio_led
@@ -623,6 +633,10 @@ void __init bcm47xx_leds_register(void)
 		bcm47xx_set_pdata(bcm47xx_leds_linksys_wrtsl54gs);
 		break;
 
+	case BCM47XX_BOARD_LUXUL_XWR_1750_V1:
+		bcm47xx_set_pdata(bcm47xx_leds_luxul_xwr_1750_v1);
+		break;
+
 	case BCM47XX_BOARD_MICROSOFT_MN700:
 		bcm47xx_set_pdata(bcm47xx_leds_microsoft_nm700);
 		break;
--- a/arch/mips/include/asm/mach-bcm47xx/bcm47xx_board.h
+++ b/arch/mips/include/asm/mach-bcm47xx/bcm47xx_board.h
@@ -80,6 +80,8 @@ enum bcm47xx_board {
 	BCM47XX_BOARD_LINKSYS_WRT610NV2,
 	BCM47XX_BOARD_LINKSYS_WRTSL54GS,
 
+	BCM47XX_BOARD_LUXUL_XWR_1750_V1,
+
 	BCM47XX_BOARD_MICROSOFT_MN700,
 
 	BCM47XX_BOARD_MOTOROLA_WE800G,
