From 01c434225ee67388711e78166cfe9b159e34fc9d Mon Sep 17 00:00:00 2001
From: Sebastian Hesselbarth <sebastian.hesselbarth@gmail.com>
Date: Fri, 19 Sep 2014 21:20:09 +0200
Subject: ARM: mvebu: armada-xp: Use pinctrl node alias

Armada XP pinctrl node gained an alias, make use of it.

Signed-off-by: Sebastian Hesselbarth <sebastian.hesselbarth@gmail.com>
Acked-by: Thomas Petazzoni <thomas.petazzoni@free-electrons.com>
Tested-By: Benoit Masson <yahoo@perenite.com>
Signed-off-by: Jason Cooper <jason@lakedaemon.net>

--- a/arch/arm/boot/dts/armada-xp-axpwifiap.dts
+++ b/arch/arm/boot/dts/armada-xp-axpwifiap.dts
@@ -60,40 +60,6 @@
 		};
 
 		internal-regs {
-			pinctrl: pin-ctrl@18000 {
-				pinctrl-0 = <&pmx_phy_int>;
-				pinctrl-names = "default";
-
-				pmx_ge0: pmx-ge0 {
-					marvell,pins = "mpp0", "mpp1", "mpp2", "mpp3",
-						       "mpp4", "mpp5", "mpp6", "mpp7",
-						       "mpp8", "mpp9", "mpp10", "mpp11";
-					marvell,function = "ge0";
-				};
-
-				pmx_ge1: pmx-ge1 {
-					marvell,pins = "mpp12", "mpp13", "mpp14", "mpp15",
-						       "mpp16", "mpp17", "mpp18", "mpp19",
-						       "mpp20", "mpp21", "mpp22", "mpp23";
-					marvell,function = "ge1";
-				};
-
-				pmx_keys: pmx-keys {
-					marvell,pins = "mpp33";
-					marvell,function = "gpio";
-				};
-
-				pmx_spi: pmx-spi {
-					marvell,pins = "mpp36", "mpp37", "mpp38", "mpp39";
-					marvell,function = "spi";
-				};
-
-				pmx_phy_int: pmx-phy-int {
-					marvell,pins = "mpp32";
-					marvell,function = "gpio";
-				};
-			};
-
 			serial@12000 {
 				status = "okay";
 			};
@@ -162,3 +128,37 @@
 		};
 	};
 };
+
+&pinctrl {
+	pinctrl-0 = <&pmx_phy_int>;
+	pinctrl-names = "default";
+
+	pmx_ge0: pmx-ge0 {
+		marvell,pins = "mpp0", "mpp1", "mpp2", "mpp3",
+			       "mpp4", "mpp5", "mpp6", "mpp7",
+			       "mpp8", "mpp9", "mpp10", "mpp11";
+		marvell,function = "ge0";
+	};
+
+	pmx_ge1: pmx-ge1 {
+		marvell,pins = "mpp12", "mpp13", "mpp14", "mpp15",
+			       "mpp16", "mpp17", "mpp18", "mpp19",
+			       "mpp20", "mpp21", "mpp22", "mpp23";
+		marvell,function = "ge1";
+	};
+
+	pmx_keys: pmx-keys {
+		marvell,pins = "mpp33";
+		marvell,function = "gpio";
+	};
+
+	pmx_spi: pmx-spi {
+		marvell,pins = "mpp36", "mpp37", "mpp38", "mpp39";
+		marvell,function = "spi";
+	};
+
+	pmx_phy_int: pmx-phy-int {
+		marvell,pins = "mpp32";
+		marvell,function = "gpio";
+	};
+};
--- a/arch/arm/boot/dts/armada-xp-lenovo-ix4-300d.dts
+++ b/arch/arm/boot/dts/armada-xp-lenovo-ix4-300d.dts
@@ -51,37 +51,6 @@
 		};
 
 		internal-regs {
-			pinctrl: pin-ctrl@18000 {
-				poweroff_pin: poweroff-pin {
-					marvell,pins = "mpp24";
-					marvell,function = "gpio";
-				};
-
-				power_button_pin: power-button-pin {
-					marvell,pins = "mpp44";
-					marvell,function = "gpio";
-				};
-
-				reset_button_pin: reset-button-pin {
-					marvell,pins = "mpp45";
-					marvell,function = "gpio";
-				};
-				select_button_pin: select-button-pin {
-					marvell,pins = "mpp41";
-					marvell,function = "gpio";
-				};
-
-				scroll_button_pin: scroll-button-pin {
-					marvell,pins = "mpp42";
-					marvell,function = "gpio";
-				};
-
-				hdd_led_pin: hdd-led-pin {
-					marvell,pins = "mpp26";
-					marvell,function = "gpio";
-				};
-			};
-
 			serial@12000 {
 				status = "okay";
 			};
@@ -282,3 +251,34 @@
 		gpios = <&gpio0 24 GPIO_ACTIVE_HIGH>;
 	};
 };
+
+&pinctrl {
+	poweroff_pin: poweroff-pin {
+		marvell,pins = "mpp24";
+		marvell,function = "gpio";
+	};
+
+	power_button_pin: power-button-pin {
+		marvell,pins = "mpp44";
+		marvell,function = "gpio";
+	};
+
+	reset_button_pin: reset-button-pin {
+		marvell,pins = "mpp45";
+		marvell,function = "gpio";
+	};
+	select_button_pin: select-button-pin {
+		marvell,pins = "mpp41";
+		marvell,function = "gpio";
+	};
+
+	scroll_button_pin: scroll-button-pin {
+		marvell,pins = "mpp42";
+		marvell,function = "gpio";
+	};
+
+	hdd_led_pin: hdd-led-pin {
+		marvell,pins = "mpp26";
+		marvell,function = "gpio";
+	};
+};
--- a/arch/arm/boot/dts/armada-xp-mv78230.dtsi
+++ b/arch/arm/boot/dts/armada-xp-mv78230.dtsi
@@ -167,10 +167,6 @@
 		};
 
 		internal-regs {
-			pinctrl: pin-ctrl@18000 {
-				compatible = "marvell,mv78230-pinctrl";
-			};
-
 			gpio0: gpio@18100 {
 				compatible = "marvell,orion-gpio";
 				reg = <0x18100 0x40>;
@@ -195,3 +191,7 @@
 		};
 	};
 };
+
+&pinctrl {
+	compatible = "marvell,mv78230-pinctrl";
+};
--- a/arch/arm/boot/dts/armada-xp-mv78260.dtsi
+++ b/arch/arm/boot/dts/armada-xp-mv78260.dtsi
@@ -251,10 +251,6 @@
 		};
 
 		internal-regs {
-			pinctrl: pin-ctrl@18000 {
-				compatible = "marvell,mv78260-pinctrl";
-			};
-
 			gpio0: gpio@18100 {
 				compatible = "marvell,orion-gpio";
 				reg = <0x18100 0x40>;
@@ -298,3 +294,7 @@
 		};
 	};
 };
+
+&pinctrl {
+	compatible = "marvell,mv78260-pinctrl";
+};
--- a/arch/arm/boot/dts/armada-xp-mv78460.dtsi
+++ b/arch/arm/boot/dts/armada-xp-mv78460.dtsi
@@ -289,10 +289,6 @@
 		};
 
 		internal-regs {
-			pinctrl: pin-ctrl@18000 {
-				compatible = "marvell,mv78460-pinctrl";
-			};
-
 			gpio0: gpio@18100 {
 				compatible = "marvell,orion-gpio";
 				reg = <0x18100 0x40>;
@@ -336,3 +332,7 @@
 		};
 	};
 };
+
+&pinctrl {
+	compatible = "marvell,mv78460-pinctrl";
+};
--- a/arch/arm/boot/dts/armada-xp-openblocks-ax3-4.dts
+++ b/arch/arm/boot/dts/armada-xp-openblocks-ax3-4.dts
@@ -81,12 +81,7 @@
 			serial@12100 {
 				status = "okay";
 			};
-			pinctrl: pin-ctrl@18000 {
-				led_pins: led-pins-0 {
-					marvell,pins = "mpp49", "mpp51", "mpp53";
-					marvell,function = "gpio";
-				};
-			};
+
 			leds {
 				compatible = "gpio-leds";
 				pinctrl-names = "default";
@@ -191,3 +186,10 @@
 		};
 	};
 };
+
+&pinctrl {
+	led_pins: led-pins-0 {
+		marvell,pins = "mpp49", "mpp51", "mpp53";
+		marvell,function = "gpio";
+	};
+};
