From 4abdde3ad6bc0b3b157c4bf6ec0bf139d11d07e8 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <zajec5@gmail.com>
Date: Wed, 13 May 2015 14:13:28 +0200
Subject: [PATCH] b53: add hacky CPU port fixes for devices not using port 5
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Signed-off-by: Rafał Miłecki <zajec5@gmail.com>
---
 drivers/net/phy/b53/b53_common.c | 6 ++++++
 1 file changed, 6 insertions(+)

--- a/drivers/net/phy/b53/b53_common.c
+++ b/drivers/net/phy/b53/b53_common.c
@@ -25,6 +25,7 @@
 #include <linux/module.h>
 #include <linux/switch.h>
 #include <linux/platform_data/b53.h>
+#include <linux/of.h>
 
 #include "b53_regs.h"
 #include "b53_priv.h"
@@ -1313,6 +1314,20 @@ static int b53_switch_init(struct b53_de
 			sw_dev->cpu_port = 5;
 	}
 
+	if (of_machine_is_compatible("asus,rt-ac87u"))
+		sw_dev->cpu_port = 7;
+	else if (of_machine_is_compatible("netgear,r8000"))
+		sw_dev->cpu_port = 8;
+	else if (of_machine_is_compatible("netgear,r8500"))
+		sw_dev->cpu_port = 8;
+
+	/*
+	 * Workaround for devices using port 8 (connected to the 3rd iface).
+	 * For some reason it doesn't work (no packets on eth2).
+	 */
+	if (of_machine_is_compatible("netgear,r8000"))
+		sw_dev->cpu_port = 5;
+
 	/* cpu port is always last */
 	sw_dev->ports = sw_dev->cpu_port + 1;
 	dev->enabled_ports |= BIT(sw_dev->cpu_port);
