From: Felix Fietkau <nbd@openwrt.org>
Date: Mon, 23 Mar 2015 02:40:06 +0100
Subject: [PATCH] bgmac: fix descriptor frame start/end definitions

The start-of-frame and end-of-frame bits were accidentally swapped.
In the current code it does not make any difference, since they are
always used together.

Signed-off-by: Felix Fietkau <nbd@openwrt.org>
---

--- a/drivers/net/ethernet/broadcom/bgmac.h
+++ b/drivers/net/ethernet/broadcom/bgmac.h
@@ -345,8 +345,8 @@
 
 #define BGMAC_DESC_CTL0_EOT			0x10000000	/* End of ring */
 #define BGMAC_DESC_CTL0_IOC			0x20000000	/* IRQ on complete */
-#define BGMAC_DESC_CTL0_SOF			0x40000000	/* Start of frame */
-#define BGMAC_DESC_CTL0_EOF			0x80000000	/* End of frame */
+#define BGMAC_DESC_CTL0_EOF			0x40000000	/* End of frame */
+#define BGMAC_DESC_CTL0_SOF			0x80000000	/* Start of frame */
 #define BGMAC_DESC_CTL1_LEN			0x00001FFF
 
 #define BGMAC_PHY_NOREGS			0x1E
