From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <zajec5@gmail.com>
Date: Sun, 7 Jun 2015 15:37:43 +0200
Subject: [PATCH] ARM: BCM5301X: Add duplicated NAND entries for bcm_nand
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

In OpenWrt we still use old NAND driver instead of "brcm,nandcs", so
we need to add this DT entry back.

Signed-off-by: Rafał Miłecki <zajec5@gmail.com>
---
--- a/arch/arm/boot/dts/bcm4708-luxul-xwc-1000.dts
+++ b/arch/arm/boot/dts/bcm4708-luxul-xwc-1000.dts
@@ -24,6 +24,18 @@
 		reg = <0x00000000 0x08000000>;
 	};
 
+	axi@18000000 {
+		nand@28000 {
+			reg = <0x00028000 0x1000>;
+			#address-cells = <1>;
+			#size-cells = <1>;
+			partition@0 {
+				label = "ubi";
+				reg = <0x00000000 0x08000000>;
+			};
+		};
+	};
+
 	nand: nand@18028000 {
 		nandcs@0 {
 			partition@0 {
--- a/arch/arm/boot/dts/bcm47094-dlink-dir-885l.dts
+++ b/arch/arm/boot/dts/bcm47094-dlink-dir-885l.dts
@@ -25,6 +25,19 @@
 		       0x88000000 0x08000000>;
 	};
 
+	axi@18000000 {
+		nand@28000 {
+			reg = <0x00028000 0x1000>;
+			#address-cells = <1>;
+			#size-cells = <1>;
+
+			partition@0 {
+				label = "firmware";
+				reg = <0x00000000 0x08000000>;
+			};
+		};
+	};
+
 	nand: nand@18028000 {
 		nandcs@0 {
 			partition@0 {
