From ffb27de4760595c356ef619c97f25722c8db28e7 Mon Sep 17 00:00:00 2001
From: John Crispin <blogic@openwrt.org>
Date: Sun, 27 Jul 2014 09:49:07 +0100
Subject: [PATCH 38/57] USB: add OHCI/EHCI OF binding

based on f3bc64d6d1f21c1b92d75f233a37b75d77af6963

Signed-off-by: John Crispin <blogic@openwrt.org>
---
 drivers/usb/Makefile             |    3 ++-
 drivers/usb/host/ehci-platform.c |   21 +++++++++++++++++----
 drivers/usb/host/ohci-platform.c |   37 +++++++++++++++++++++++++++++++------
 3 files changed, 50 insertions(+), 11 deletions(-)

--- a/drivers/usb/host/ehci-platform.c
+++ b/drivers/usb/host/ehci-platform.c
@@ -359,6 +359,7 @@ static int ehci_platform_resume(struct d
 static const struct of_device_id vt8500_ehci_ids[] = {
 	{ .compatible = "via,vt8500-ehci", },
 	{ .compatible = "wm,prizm-ehci", },
+	{ .compatible = "ralink,rt3xxx-ehci", },
 	{ .compatible = "generic-ehci", },
 	{}
 };
--- a/drivers/usb/host/ohci-platform.c
+++ b/drivers/usb/host/ohci-platform.c
@@ -342,6 +342,7 @@ static int ohci_platform_resume(struct d
 #endif /* CONFIG_PM */
 
 static const struct of_device_id ohci_platform_ids[] = {
+	{ .compatible = "ralink,rt3xxx-ohci", },
 	{ .compatible = "generic-ohci", },
 	{ }
 };
