From 26305d3d7298d1ddf8fd4ce95a382aa90534f0a3 Mon Sep 17 00:00:00 2001
From: Arend Van Spriel <arend.vanspriel@broadcom.com>
Date: Mon, 19 Sep 2016 12:09:54 +0100
Subject: [PATCH] brcmfmac: initialize variable in brcmf_sdiod_regrl()

In case of an error the variable returned is uninitialized. The caller
will probably check the error code before using it, but better assure
it is set to zero.

Reviewed-by: Hante Meuleman <hante.meuleman@broadcom.com>
Reviewed-by: Pieter-Paul Giesberts <pieter-paul.giesberts@broadcom.com>
Signed-off-by: Arend van Spriel <arend.vanspriel@broadcom.com>
Signed-off-by: Kalle Valo <kvalo@codeaurora.org>
---
 drivers/net/wireless/broadcom/brcm80211/brcmfmac/bcmsdh.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/net/wireless/broadcom/brcm80211/brcmfmac/bcmsdh.c
+++ b/drivers/net/wireless/broadcom/brcm80211/brcmfmac/bcmsdh.c
@@ -416,7 +416,7 @@ u8 brcmf_sdiod_regrb(struct brcmf_sdio_d
 
 u32 brcmf_sdiod_regrl(struct brcmf_sdio_dev *sdiodev, u32 addr, int *ret)
 {
-	u32 data;
+	u32 data = 0;
 	int retval;
 
 	brcmf_dbg(SDIO, "addr:0x%08x\n", addr);
