From b7e4d148906685882a081e7e50692313c5a8724e Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <zajec5@gmail.com>
Date: Wed, 1 Oct 2014 09:23:09 +0200
Subject: [PATCH 2/2] ARM: BCM5301X: Add LEDs for Netgear R6250 V1
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Signed-off-by: Rafał Miłecki <zajec5@gmail.com>
---
 arch/arm/boot/dts/bcm4708-netgear-r6250.dts | 34 +++++++++++++++++++++++++++++
 1 file changed, 34 insertions(+)

--- a/arch/arm/boot/dts/bcm4708-netgear-r6250.dts
+++ b/arch/arm/boot/dts/bcm4708-netgear-r6250.dts
@@ -32,4 +32,38 @@
 			status = "okay";
 		};
 	};
+
+	leds {
+		compatible = "gpio-leds";
+
+		logo {
+			label = "bcm53xx:white:logo";
+			gpios = <&chipcommon 1 GPIO_ACTIVE_HIGH>;
+			linux,default-trigger = "default-on";
+		};
+
+		power0 {
+			label = "bcm53xx:green:power";
+			gpios = <&chipcommon 2 GPIO_ACTIVE_LOW>;
+			linux,default-trigger = "default-off";
+		};
+
+		power1 {
+			label = "bcm53xx:amber:power";
+			gpios = <&chipcommon 3 GPIO_ACTIVE_LOW>;
+			linux,default-trigger = "default-on";
+		};
+
+		usb {
+			label = "bcm53xx:blue:usb";
+			gpios = <&chipcommon 8 GPIO_ACTIVE_LOW>;
+			linux,default-trigger = "default-off";
+		};
+
+		wireless {
+			label = "bcm53xx:blue:wireless";
+			gpios = <&chipcommon 11 GPIO_ACTIVE_LOW>;
+			linux,default-trigger = "default-off";
+		};
+	};
 };
