From: Ezequiel Garcia <ezequiel.garcia@free-electrons.com>
Subject: [PATCH] net: mv643xx_eth: Make TSO disabled by default

Data corruption has been observed to be produced by TSO. For instance,
accessing files on a NFS-server with TSO enabled results in different data
transferred each time.

This has been observed only on Kirkwood platforms, i.e. with the mv643xx_eth
driver. Same tests on platforms using the mvneta ethernet driver have
passed without errors.

Make TSO disabled by default for now, until we can found a proper fix
for the regression.

Fixes: 3ae8f4e0b98 ('net: mv643xx_eth: Implement software TSO')
Reported-by: Slawomir Gajzner <slawomir.gajzner <at> gmail.com>
Reported-by: Julien D'Ascenzio <jdascenzio <at> yahoo.fr>
Signed-off-by: Ezequiel Garcia <ezequiel.garcia <at> free-electrons.com>
---
--- a/drivers/net/ethernet/marvell/mv643xx_eth.c
+++ b/drivers/net/ethernet/marvell/mv643xx_eth.c
@@ -3112,11 +3112,11 @@ static int mv643xx_eth_probe(struct plat
 	dev->watchdog_timeo = 2 * HZ;
 	dev->base_addr = 0;
 
-	dev->features = NETIF_F_SG | NETIF_F_IP_CSUM | NETIF_F_TSO;
+	dev->features = NETIF_F_SG | NETIF_F_IP_CSUM;
 	dev->vlan_features = dev->features;
 
 	dev->features |= NETIF_F_RXCSUM;
-	dev->hw_features = dev->features;
+	dev->hw_features = dev->features | NETIF_F_TSO;
 
 	dev->priv_flags |= IFF_UNICAST_FLT;
 	dev->gso_max_segs = MV643XX_MAX_TSO_SEGS;
