#!/bin/sh
#
# Copyright (C) 2013-2014 OpenWrt.org
#

[ -e /etc/config/network ] && exit 0

touch /etc/config/network

. /lib/sunxi.sh
. /lib/functions/uci-defaults.sh

ucidef_set_interface_loopback

case "$( sunxi_board_name )" in
"olinuxino-micro"*)
	ucidef_set_interface_lan 'wlan0'
	;;
"lamobo-r1")
	ucidef_set_interfaces_lan_wan "eth0.1" "eth0.2"
	ucidef_add_switch "switch0" "1" "1"
	ucidef_add_switch_vlan "switch0" "1" "4 0 1 2 8t"
	ucidef_add_switch_vlan "switch0" "2" "3 8t"
	;;
*)
	ucidef_set_interface_lan 'eth0'
	;;
esac

uci commit network

exit 0
