--- a/arch/mips/bcm47xx/board.c
+++ b/arch/mips/bcm47xx/board.c
@@ -140,6 +140,7 @@ struct bcm47xx_board_type_list2 bcm47xx_
 	{{BCM47XX_BOARD_LINKSYS_WRT300NV11, "Linksys WRT300N V1.1"}, "WRT300N", "1.1"},
 	{{BCM47XX_BOARD_LINKSYS_WRT310NV1, "Linksys WRT310N V1"}, "WRT310N", "1.0"},
 	{{BCM47XX_BOARD_LINKSYS_WRT310NV2, "Linksys WRT310N V2"}, "WRT310N", "2.0"},
+	{{BCM47XX_BOARD_LINKSYS_WRT320N_V1, "Linksys WRT320N V1"}, "WRT320N", "1.0"},
 	{{BCM47XX_BOARD_LINKSYS_WRT54G3GV2, "Linksys WRT54G3GV2-VF"}, "WRT54G3GV2-VF", "1.0"},
 	{{BCM47XX_BOARD_LINKSYS_WRT610NV1, "Linksys WRT610N V1"}, "WRT610N", "1.0"},
 	{{BCM47XX_BOARD_LINKSYS_WRT610NV2, "Linksys WRT610N V2"}, "WRT610N", "2.0"},
@@ -162,6 +163,7 @@ struct bcm47xx_board_type_list1 bcm47xx_
 	{{BCM47XX_BOARD_NETGEAR_WNDR4000, "Netgear WNDR4000"}, "U12H181T00_NETGEAR"},
 	{{BCM47XX_BOARD_NETGEAR_WNDR4500V1, "Netgear WNDR4500 V1"}, "U12H189T00_NETGEAR"},
 	{{BCM47XX_BOARD_NETGEAR_WNDR4500V2, "Netgear WNDR4500 V2"}, "U12H224T00_NETGEAR"},
+	{{BCM47XX_BOARD_NETGEAR_WNR1000_V3, "Netgear WNR1000 V3"}, "U12H139T50_NETGEAR"},
 	{{BCM47XX_BOARD_NETGEAR_WNR2000, "Netgear WNR2000"}, "U12H114T00_NETGEAR"},
 	{{BCM47XX_BOARD_NETGEAR_WNR3500L, "Netgear WNR3500L"}, "U12H136T99_NETGEAR"},
 	{{BCM47XX_BOARD_NETGEAR_WNR3500U, "Netgear WNR3500U"}, "U12H136T00_NETGEAR"},
--- a/arch/mips/bcm47xx/buttons.c
+++ b/arch/mips/bcm47xx/buttons.c
@@ -20,6 +20,12 @@
 /* Asus */
 
 static const struct gpio_keys_button
+bcm47xx_buttons_asus_rtn10u[] __initconst = {
+	BCM47XX_GPIO_KEY(20, KEY_WPS_BUTTON),
+	BCM47XX_GPIO_KEY(21, KEY_RESTART),
+};
+
+static const struct gpio_keys_button
 bcm47xx_buttons_asus_rtn12[] __initconst = {
 	BCM47XX_GPIO_KEY(0, KEY_WPS_BUTTON),
 	BCM47XX_GPIO_KEY(1, KEY_RESTART),
@@ -270,6 +276,18 @@ bcm47xx_buttons_linksys_wrt310nv1[] __in
 };
 
 static const struct gpio_keys_button
+bcm47xx_buttons_linksys_wrt310n_v2[] __initconst = {
+	BCM47XX_GPIO_KEY(5, KEY_WPS_BUTTON),
+	BCM47XX_GPIO_KEY(6, KEY_RESTART),
+};
+
+static const struct gpio_keys_button
+bcm47xx_buttons_linksys_wrt320n_v1[] __initconst = {
+	BCM47XX_GPIO_KEY(5, KEY_WPS_BUTTON),
+	BCM47XX_GPIO_KEY(8, KEY_RESTART),
+};
+
+static const struct gpio_keys_button
 bcm47xx_buttons_linksys_wrt54g3gv2[] __initconst = {
 	BCM47XX_GPIO_KEY(5, KEY_WIMAX),
 	BCM47XX_GPIO_KEY(6, KEY_RESTART),
@@ -360,6 +378,11 @@ bcm47xx_buttons_netgear_wndr4500v1[] __i
 };
 
 static const struct gpio_keys_button
+bcm47xx_buttons_netgear_wnr1000_v3[] __initconst = {
+	BCM47XX_GPIO_KEY(3, KEY_RESTART),
+};
+
+static const struct gpio_keys_button
 bcm47xx_buttons_netgear_wnr3500lv1[] __initconst = {
 	BCM47XX_GPIO_KEY(4, KEY_RESTART),
 	BCM47XX_GPIO_KEY(6, KEY_WPS_BUTTON),
@@ -414,6 +437,9 @@ int __init bcm47xx_buttons_register(void
 	int err;
 
 	switch (board) {
+	case BCM47XX_BOARD_ASUS_RTN10U:
+		err = bcm47xx_copy_bdata(bcm47xx_buttons_asus_rtn10u);
+		break;
 	case BCM47XX_BOARD_ASUS_RTN12:
 		err = bcm47xx_copy_bdata(bcm47xx_buttons_asus_rtn12);
 		break;
@@ -544,6 +570,12 @@ int __init bcm47xx_buttons_register(void
 	case BCM47XX_BOARD_LINKSYS_WRT310NV1:
 		err = bcm47xx_copy_bdata(bcm47xx_buttons_linksys_wrt310nv1);
 		break;
+	case BCM47XX_BOARD_LINKSYS_WRT310NV2:
+		err = bcm47xx_copy_bdata(bcm47xx_buttons_linksys_wrt310n_v2);
+		break;
+	case BCM47XX_BOARD_LINKSYS_WRT320N_V1:
+		err = bcm47xx_copy_bdata(bcm47xx_buttons_linksys_wrt320n_v1);
+		break;
 	case BCM47XX_BOARD_LINKSYS_WRT54G3GV2:
 		err = bcm47xx_copy_bdata(bcm47xx_buttons_linksys_wrt54g3gv2);
 		break;
@@ -592,6 +624,9 @@ int __init bcm47xx_buttons_register(void
 	case BCM47XX_BOARD_NETGEAR_WNDR4500V1:
 		err = bcm47xx_copy_bdata(bcm47xx_buttons_netgear_wndr4500v1);
 		break;
+	case BCM47XX_BOARD_NETGEAR_WNR1000_V3:
+		err = bcm47xx_copy_bdata(bcm47xx_buttons_netgear_wnr1000_v3);
+		break;
 	case BCM47XX_BOARD_NETGEAR_WNR3500L:
 		err = bcm47xx_copy_bdata(bcm47xx_buttons_netgear_wnr3500lv1);
 		break;
--- a/arch/mips/include/asm/mach-bcm47xx/bcm47xx_board.h
+++ b/arch/mips/include/asm/mach-bcm47xx/bcm47xx_board.h
@@ -71,6 +71,7 @@ enum bcm47xx_board {
 	BCM47XX_BOARD_LINKSYS_WRT300NV11,
 	BCM47XX_BOARD_LINKSYS_WRT310NV1,
 	BCM47XX_BOARD_LINKSYS_WRT310NV2,
+	BCM47XX_BOARD_LINKSYS_WRT320N_V1,
 	BCM47XX_BOARD_LINKSYS_WRT54G3GV2,
 	BCM47XX_BOARD_LINKSYS_WRT54G_TYPE_0101,
 	BCM47XX_BOARD_LINKSYS_WRT54G_TYPE_0467,
@@ -100,6 +101,7 @@ enum bcm47xx_board {
 	BCM47XX_BOARD_NETGEAR_WNDR4000,
 	BCM47XX_BOARD_NETGEAR_WNDR4500V1,
 	BCM47XX_BOARD_NETGEAR_WNDR4500V2,
+	BCM47XX_BOARD_NETGEAR_WNR1000_V3,
 	BCM47XX_BOARD_NETGEAR_WNR2000,
 	BCM47XX_BOARD_NETGEAR_WNR3500L,
 	BCM47XX_BOARD_NETGEAR_WNR3500U,
--- a/arch/mips/bcm47xx/leds.c
+++ b/arch/mips/bcm47xx/leds.c
@@ -29,6 +29,14 @@
 /* Asus */
 
 static const struct gpio_led
+bcm47xx_leds_asus_rtn10u[] __initconst = {
+	BCM47XX_GPIO_LED(5, "green", "wlan", 0, LEDS_GPIO_DEFSTATE_OFF),
+	BCM47XX_GPIO_LED(6, "green", "power", 1, LEDS_GPIO_DEFSTATE_ON),
+	BCM47XX_GPIO_LED(7, "green", "wps", 0, LEDS_GPIO_DEFSTATE_OFF),
+	BCM47XX_GPIO_LED(8, "green", "usb", 0, LEDS_GPIO_DEFSTATE_OFF),
+};
+
+static const struct gpio_led
 bcm47xx_leds_asus_rtn12[] __initconst = {
 	BCM47XX_GPIO_LED(2, "unk", "power", 1, LEDS_GPIO_DEFSTATE_ON),
 	BCM47XX_GPIO_LED(7, "unk", "wlan", 0, LEDS_GPIO_DEFSTATE_OFF),
@@ -313,6 +321,13 @@ bcm47xx_leds_linksys_wrt310nv1[] __initc
 };
 
 static const struct gpio_led
+bcm47xx_leds_linksys_wrt320n_v1[] __initconst = {
+	BCM47XX_GPIO_LED(1, "blue", "wlan", 1, LEDS_GPIO_DEFSTATE_OFF),
+	BCM47XX_GPIO_LED(2, "blue", "power", 0, LEDS_GPIO_DEFSTATE_ON),
+	BCM47XX_GPIO_LED(4, "amber", "wps", 1, LEDS_GPIO_DEFSTATE_OFF),
+};
+
+static const struct gpio_led
 bcm47xx_leds_linksys_wrt54g_generic[] __initconst = {
 	BCM47XX_GPIO_LED(0, "unk", "dmz", 1, LEDS_GPIO_DEFSTATE_OFF),
 	BCM47XX_GPIO_LED(1, "unk", "power", 0, LEDS_GPIO_DEFSTATE_ON),
@@ -478,6 +493,9 @@ void __init bcm47xx_leds_register(void)
 	enum bcm47xx_board board = bcm47xx_board_get();
 
 	switch (board) {
+	case BCM47XX_BOARD_ASUS_RTN10U:
+		bcm47xx_set_pdata(bcm47xx_leds_asus_rtn10u);
+		break;
 	case BCM47XX_BOARD_ASUS_RTN12:
 		bcm47xx_set_pdata(bcm47xx_leds_asus_rtn12);
 		break;
@@ -611,6 +629,9 @@ void __init bcm47xx_leds_register(void)
 	case BCM47XX_BOARD_LINKSYS_WRT310NV1:
 		bcm47xx_set_pdata(bcm47xx_leds_linksys_wrt310nv1);
 		break;
+	case BCM47XX_BOARD_LINKSYS_WRT320N_V1:
+		bcm47xx_set_pdata(bcm47xx_leds_linksys_wrt320n_v1);
+		break;
 	case BCM47XX_BOARD_LINKSYS_WRT54G3GV2:
 		bcm47xx_set_pdata(bcm47xx_leds_linksys_wrt54g3gv2);
 		break;
