From 6d668fef3a1baa60bdd715ee062ddb6333d2647c Mon Sep 17 00:00:00 2001
From: Gabor Juhos <juhosg@openwrt.org>
Date: Mon, 30 Sep 2013 16:58:23 +0200
Subject: [PATCH] rt2x00: rt2800lib: fix LNA gain configuration for RT3883

Signed-off-by: Gabor Juhos <juhosg@openwrt.org>
---
 drivers/net/wireless/ralink/rt2x00/rt2800lib.c |    6 ++++--
 1 file changed, 4 insertions(+), 2 deletions(-)

--- a/drivers/net/wireless/ralink/rt2x00/rt2800lib.c
+++ b/drivers/net/wireless/ralink/rt2x00/rt2800lib.c
@@ -1961,7 +1961,8 @@ static void rt2800_config_lna_gain(struc
 		rt2800_eeprom_read(rt2x00dev, EEPROM_LNA, &eeprom);
 		lna_gain = rt2x00_get_field16(eeprom, EEPROM_LNA_A0);
 	} else if (libconf->rf.channel <= 128) {
-		if (rt2x00_rt(rt2x00dev, RT3593)) {
+		if (rt2x00_rt(rt2x00dev, RT3593) ||
+		    rt2x00_rt(rt2x00dev, RT3883)) {
 			rt2800_eeprom_read(rt2x00dev, EEPROM_EXT_LNA2, &eeprom);
 			lna_gain = rt2x00_get_field16(eeprom,
 						      EEPROM_EXT_LNA2_A1);
@@ -1971,7 +1972,8 @@ static void rt2800_config_lna_gain(struc
 						      EEPROM_RSSI_BG2_LNA_A1);
 		}
 	} else {
-		if (rt2x00_rt(rt2x00dev, RT3593)) {
+		if (rt2x00_rt(rt2x00dev, RT3593) ||
+		    rt2x00_rt(rt2x00dev, RT3883)) {
 			rt2800_eeprom_read(rt2x00dev, EEPROM_EXT_LNA2, &eeprom);
 			lna_gain = rt2x00_get_field16(eeprom,
 						      EEPROM_EXT_LNA2_A2);
