--- a/drivers/bcma/driver_chipcommon.c
+++ b/drivers/bcma/driver_chipcommon.c
@@ -15,6 +15,8 @@
 #include <linux/platform_device.h>
 #include <linux/bcma/bcma.h>
 
+static void bcma_chipco_serial_init(struct bcma_drv_cc *cc);
+
 static inline u32 bcma_cc_write32_masked(struct bcma_drv_cc *cc, u16 offset,
 					 u32 mask, u32 value)
 {
@@ -115,6 +117,8 @@ int bcma_chipco_watchdog_register(struct
 
 void bcma_core_chipcommon_early_init(struct bcma_drv_cc *cc)
 {
+	struct bcma_bus *bus = cc->core->bus;
+
 	if (cc->early_setup_done)
 		return;
 
@@ -129,6 +133,9 @@ void bcma_core_chipcommon_early_init(str
 	if (cc->capabilities & BCMA_CC_CAP_PMU)
 		bcma_pmu_early_init(cc);
 
+	if (IS_BUILTIN(CONFIG_BCM47XX) && bus->hosttype == BCMA_HOSTTYPE_SOC)
+		bcma_chipco_serial_init(cc);
+
 	cc->early_setup_done = true;
 }
 
@@ -185,11 +192,12 @@ u32 bcma_chipco_watchdog_timer_set(struc
 			ticks = 2;
 		else if (ticks > maxt)
 			ticks = maxt;
-		bcma_cc_write32(cc, BCMA_CC_PMU_WATCHDOG, ticks);
+		bcma_pmu_write32(cc, BCMA_CC_PMU_WATCHDOG, ticks);
 	} else {
 		struct bcma_bus *bus = cc->core->bus;
 
 		if (bus->chipinfo.id != BCMA_CHIP_ID_BCM4707 &&
+		    bus->chipinfo.id != BCMA_CHIP_ID_BCM47094 &&
 		    bus->chipinfo.id != BCMA_CHIP_ID_BCM53018)
 			bcma_core_set_clockmode(cc->core,
 						ticks ? BCMA_CLKMODE_FAST : BCMA_CLKMODE_DYNAMIC);
@@ -314,9 +322,9 @@ u32 bcma_chipco_gpio_pulldown(struct bcm
 	return res;
 }
 
-#ifdef CONFIG_BCMA_DRIVER_MIPS
-void bcma_chipco_serial_init(struct bcma_drv_cc *cc)
+static void bcma_chipco_serial_init(struct bcma_drv_cc *cc)
 {
+#if IS_BUILTIN(CONFIG_BCM47XX)
 	unsigned int irq;
 	u32 baud_base;
 	u32 i;
@@ -358,5 +366,5 @@ void bcma_chipco_serial_init(struct bcma
 		ports[i].baud_base = baud_base;
 		ports[i].reg_shift = 0;
 	}
+#endif /* CONFIG_BCM47XX */
 }
-#endif /* CONFIG_BCMA_DRIVER_MIPS */
--- a/drivers/bcma/driver_chipcommon_pmu.c
+++ b/drivers/bcma/driver_chipcommon_pmu.c
@@ -15,44 +15,44 @@
 
 u32 bcma_chipco_pll_read(struct bcma_drv_cc *cc, u32 offset)
 {
-	bcma_cc_write32(cc, BCMA_CC_PLLCTL_ADDR, offset);
-	bcma_cc_read32(cc, BCMA_CC_PLLCTL_ADDR);
-	return bcma_cc_read32(cc, BCMA_CC_PLLCTL_DATA);
+	bcma_pmu_write32(cc, BCMA_CC_PMU_PLLCTL_ADDR, offset);
+	bcma_pmu_read32(cc, BCMA_CC_PMU_PLLCTL_ADDR);
+	return bcma_pmu_read32(cc, BCMA_CC_PMU_PLLCTL_DATA);
 }
 EXPORT_SYMBOL_GPL(bcma_chipco_pll_read);
 
 void bcma_chipco_pll_write(struct bcma_drv_cc *cc, u32 offset, u32 value)
 {
-	bcma_cc_write32(cc, BCMA_CC_PLLCTL_ADDR, offset);
-	bcma_cc_read32(cc, BCMA_CC_PLLCTL_ADDR);
-	bcma_cc_write32(cc, BCMA_CC_PLLCTL_DATA, value);
+	bcma_pmu_write32(cc, BCMA_CC_PMU_PLLCTL_ADDR, offset);
+	bcma_pmu_read32(cc, BCMA_CC_PMU_PLLCTL_ADDR);
+	bcma_pmu_write32(cc, BCMA_CC_PMU_PLLCTL_DATA, value);
 }
 EXPORT_SYMBOL_GPL(bcma_chipco_pll_write);
 
 void bcma_chipco_pll_maskset(struct bcma_drv_cc *cc, u32 offset, u32 mask,
 			     u32 set)
 {
-	bcma_cc_write32(cc, BCMA_CC_PLLCTL_ADDR, offset);
-	bcma_cc_read32(cc, BCMA_CC_PLLCTL_ADDR);
-	bcma_cc_maskset32(cc, BCMA_CC_PLLCTL_DATA, mask, set);
+	bcma_pmu_write32(cc, BCMA_CC_PMU_PLLCTL_ADDR, offset);
+	bcma_pmu_read32(cc, BCMA_CC_PMU_PLLCTL_ADDR);
+	bcma_pmu_maskset32(cc, BCMA_CC_PMU_PLLCTL_DATA, mask, set);
 }
 EXPORT_SYMBOL_GPL(bcma_chipco_pll_maskset);
 
 void bcma_chipco_chipctl_maskset(struct bcma_drv_cc *cc,
 				 u32 offset, u32 mask, u32 set)
 {
-	bcma_cc_write32(cc, BCMA_CC_CHIPCTL_ADDR, offset);
-	bcma_cc_read32(cc, BCMA_CC_CHIPCTL_ADDR);
-	bcma_cc_maskset32(cc, BCMA_CC_CHIPCTL_DATA, mask, set);
+	bcma_pmu_write32(cc, BCMA_CC_PMU_CHIPCTL_ADDR, offset);
+	bcma_pmu_read32(cc, BCMA_CC_PMU_CHIPCTL_ADDR);
+	bcma_pmu_maskset32(cc, BCMA_CC_PMU_CHIPCTL_DATA, mask, set);
 }
 EXPORT_SYMBOL_GPL(bcma_chipco_chipctl_maskset);
 
 void bcma_chipco_regctl_maskset(struct bcma_drv_cc *cc, u32 offset, u32 mask,
 				u32 set)
 {
-	bcma_cc_write32(cc, BCMA_CC_REGCTL_ADDR, offset);
-	bcma_cc_read32(cc, BCMA_CC_REGCTL_ADDR);
-	bcma_cc_maskset32(cc, BCMA_CC_REGCTL_DATA, mask, set);
+	bcma_pmu_write32(cc, BCMA_CC_PMU_REGCTL_ADDR, offset);
+	bcma_pmu_read32(cc, BCMA_CC_PMU_REGCTL_ADDR);
+	bcma_pmu_maskset32(cc, BCMA_CC_PMU_REGCTL_DATA, mask, set);
 }
 EXPORT_SYMBOL_GPL(bcma_chipco_regctl_maskset);
 
@@ -60,18 +60,18 @@ static u32 bcma_pmu_xtalfreq(struct bcma
 {
 	u32 ilp_ctl, alp_hz;
 
-	if (!(bcma_cc_read32(cc, BCMA_CC_PMU_STAT) &
+	if (!(bcma_pmu_read32(cc, BCMA_CC_PMU_STAT) &
 	      BCMA_CC_PMU_STAT_EXT_LPO_AVAIL))
 		return 0;
 
-	bcma_cc_write32(cc, BCMA_CC_PMU_XTAL_FREQ,
-			BIT(BCMA_CC_PMU_XTAL_FREQ_MEASURE_SHIFT));
+	bcma_pmu_write32(cc, BCMA_CC_PMU_XTAL_FREQ,
+			 BIT(BCMA_CC_PMU_XTAL_FREQ_MEASURE_SHIFT));
 	usleep_range(1000, 2000);
 
-	ilp_ctl = bcma_cc_read32(cc, BCMA_CC_PMU_XTAL_FREQ);
+	ilp_ctl = bcma_pmu_read32(cc, BCMA_CC_PMU_XTAL_FREQ);
 	ilp_ctl &= BCMA_CC_PMU_XTAL_FREQ_ILPCTL_MASK;
 
-	bcma_cc_write32(cc, BCMA_CC_PMU_XTAL_FREQ, 0);
+	bcma_pmu_write32(cc, BCMA_CC_PMU_XTAL_FREQ, 0);
 
 	alp_hz = ilp_ctl * 32768 / 4;
 	return (alp_hz + 50000) / 100000 * 100;
@@ -127,8 +127,8 @@ static void bcma_pmu2_pll_init0(struct b
 		mask = (u32)~(BCMA_RES_4314_HT_AVAIL |
 			      BCMA_RES_4314_MACPHY_CLK_AVAIL);
 
-		bcma_cc_mask32(cc, BCMA_CC_PMU_MINRES_MSK, mask);
-		bcma_cc_mask32(cc, BCMA_CC_PMU_MAXRES_MSK, mask);
+		bcma_pmu_mask32(cc, BCMA_CC_PMU_MINRES_MSK, mask);
+		bcma_pmu_mask32(cc, BCMA_CC_PMU_MAXRES_MSK, mask);
 		bcma_wait_value(cc->core, BCMA_CLKCTLST,
 				BCMA_CLKCTLST_HAVEHT, 0, 20000);
 		break;
@@ -140,7 +140,7 @@ static void bcma_pmu2_pll_init0(struct b
 
 	/* Flush */
 	if (cc->pmu.rev >= 2)
-		bcma_cc_set32(cc, BCMA_CC_PMU_CTL, BCMA_CC_PMU_CTL_PLL_UPD);
+		bcma_pmu_set32(cc, BCMA_CC_PMU_CTL, BCMA_CC_PMU_CTL_PLL_UPD);
 
 	/* TODO: Do we need to update OTP? */
 }
@@ -195,9 +195,9 @@ static void bcma_pmu_resources_init(stru
 
 	/* Set the resource masks. */
 	if (min_msk)
-		bcma_cc_write32(cc, BCMA_CC_PMU_MINRES_MSK, min_msk);
+		bcma_pmu_write32(cc, BCMA_CC_PMU_MINRES_MSK, min_msk);
 	if (max_msk)
-		bcma_cc_write32(cc, BCMA_CC_PMU_MAXRES_MSK, max_msk);
+		bcma_pmu_write32(cc, BCMA_CC_PMU_MAXRES_MSK, max_msk);
 
 	/*
 	 * Add some delay; allow resources to come up and settle.
@@ -269,23 +269,33 @@ static void bcma_pmu_workarounds(struct
 
 void bcma_pmu_early_init(struct bcma_drv_cc *cc)
 {
+	struct bcma_bus *bus = cc->core->bus;
 	u32 pmucap;
 
-	pmucap = bcma_cc_read32(cc, BCMA_CC_PMU_CAP);
+	if (cc->core->id.rev >= 35 &&
+	    cc->capabilities_ext & BCMA_CC_CAP_EXT_AOB_PRESENT) {
+		cc->pmu.core = bcma_find_core(bus, BCMA_CORE_PMU);
+		if (!cc->pmu.core)
+			bcma_warn(bus, "Couldn't find expected PMU core");
+	}
+	if (!cc->pmu.core)
+		cc->pmu.core = cc->core;
+
+	pmucap = bcma_pmu_read32(cc, BCMA_CC_PMU_CAP);
 	cc->pmu.rev = (pmucap & BCMA_CC_PMU_CAP_REVISION);
 
-	bcma_debug(cc->core->bus, "Found rev %u PMU (capabilities 0x%08X)\n",
-		   cc->pmu.rev, pmucap);
+	bcma_debug(bus, "Found rev %u PMU (capabilities 0x%08X)\n", cc->pmu.rev,
+		   pmucap);
 }
 
 void bcma_pmu_init(struct bcma_drv_cc *cc)
 {
 	if (cc->pmu.rev == 1)
-		bcma_cc_mask32(cc, BCMA_CC_PMU_CTL,
-			      ~BCMA_CC_PMU_CTL_NOILPONW);
+		bcma_pmu_mask32(cc, BCMA_CC_PMU_CTL,
+				~BCMA_CC_PMU_CTL_NOILPONW);
 	else
-		bcma_cc_set32(cc, BCMA_CC_PMU_CTL,
-			     BCMA_CC_PMU_CTL_NOILPONW);
+		bcma_pmu_set32(cc, BCMA_CC_PMU_CTL,
+			       BCMA_CC_PMU_CTL_NOILPONW);
 
 	bcma_pmu_pll_init(cc);
 	bcma_pmu_resources_init(cc);
@@ -472,8 +482,8 @@ u32 bcma_pmu_get_cpu_clock(struct bcma_d
 static void bcma_pmu_spuravoid_pll_write(struct bcma_drv_cc *cc, u32 offset,
 					 u32 value)
 {
-	bcma_cc_write32(cc, BCMA_CC_PLLCTL_ADDR, offset);
-	bcma_cc_write32(cc, BCMA_CC_PLLCTL_DATA, value);
+	bcma_pmu_write32(cc, BCMA_CC_PMU_PLLCTL_ADDR, offset);
+	bcma_pmu_write32(cc, BCMA_CC_PMU_PLLCTL_DATA, value);
 }
 
 void bcma_pmu_spuravoid_pllupdate(struct bcma_drv_cc *cc, int spuravoid)
@@ -497,20 +507,20 @@ void bcma_pmu_spuravoid_pllupdate(struct
 		       bus->chipinfo.id == BCMA_CHIP_ID_BCM53572) ? 6 : 0;
 
 		/* RMW only the P1 divider */
-		bcma_cc_write32(cc, BCMA_CC_PLLCTL_ADDR,
+		bcma_pmu_write32(cc, BCMA_CC_PMU_PLLCTL_ADDR,
 				BCMA_CC_PMU_PLL_CTL0 + phypll_offset);
-		tmp = bcma_cc_read32(cc, BCMA_CC_PLLCTL_DATA);
+		tmp = bcma_pmu_read32(cc, BCMA_CC_PMU_PLLCTL_DATA);
 		tmp &= (~(BCMA_CC_PMU1_PLL0_PC0_P1DIV_MASK));
 		tmp |= (bcm5357_bcm43236_p1div[spuravoid] << BCMA_CC_PMU1_PLL0_PC0_P1DIV_SHIFT);
-		bcma_cc_write32(cc, BCMA_CC_PLLCTL_DATA, tmp);
+		bcma_pmu_write32(cc, BCMA_CC_PMU_PLLCTL_DATA, tmp);
 
 		/* RMW only the int feedback divider */
-		bcma_cc_write32(cc, BCMA_CC_PLLCTL_ADDR,
+		bcma_pmu_write32(cc, BCMA_CC_PMU_PLLCTL_ADDR,
 				BCMA_CC_PMU_PLL_CTL2 + phypll_offset);
-		tmp = bcma_cc_read32(cc, BCMA_CC_PLLCTL_DATA);
+		tmp = bcma_pmu_read32(cc, BCMA_CC_PMU_PLLCTL_DATA);
 		tmp &= ~(BCMA_CC_PMU1_PLL0_PC2_NDIV_INT_MASK);
 		tmp |= (bcm5357_bcm43236_ndiv[spuravoid]) << BCMA_CC_PMU1_PLL0_PC2_NDIV_INT_SHIFT;
-		bcma_cc_write32(cc, BCMA_CC_PLLCTL_DATA, tmp);
+		bcma_pmu_write32(cc, BCMA_CC_PMU_PLLCTL_DATA, tmp);
 
 		tmp = BCMA_CC_PMU_CTL_PLL_UPD;
 		break;
@@ -646,7 +656,7 @@ void bcma_pmu_spuravoid_pllupdate(struct
 		break;
 	}
 
-	tmp |= bcma_cc_read32(cc, BCMA_CC_PMU_CTL);
-	bcma_cc_write32(cc, BCMA_CC_PMU_CTL, tmp);
+	tmp |= bcma_pmu_read32(cc, BCMA_CC_PMU_CTL);
+	bcma_pmu_write32(cc, BCMA_CC_PMU_CTL, tmp);
 }
 EXPORT_SYMBOL_GPL(bcma_pmu_spuravoid_pllupdate);
--- a/drivers/bcma/driver_chipcommon_sflash.c
+++ b/drivers/bcma/driver_chipcommon_sflash.c
@@ -38,6 +38,7 @@ static const struct bcma_sflash_tbl_e bc
 	{ "M25P32", 0x15, 0x10000, 64, },
 	{ "M25P64", 0x16, 0x10000, 128, },
 	{ "M25FL128", 0x17, 0x10000, 256, },
+	{ "MX25L25635F", 0x18, 0x10000, 512, },
 	{ NULL },
 };
 
--- a/drivers/bcma/scan.c
+++ b/drivers/bcma/scan.c
@@ -98,6 +98,9 @@ static const struct bcma_device_id_name
 	{ BCMA_CORE_SHIM, "SHIM" },
 	{ BCMA_CORE_PCIE2, "PCIe Gen2" },
 	{ BCMA_CORE_ARM_CR4, "ARM CR4" },
+	{ BCMA_CORE_GCI, "GCI" },
+	{ BCMA_CORE_CMEM, "CNDS DDR2/3 memory controller" },
+	{ BCMA_CORE_ARM_CA7, "ARM CA7" },
 	{ BCMA_CORE_DEFAULT, "Default" },
 };
 
@@ -315,6 +318,8 @@ static int bcma_get_next_core(struct bcm
 		switch (core->id.id) {
 		case BCMA_CORE_4706_MAC_GBIT_COMMON:
 		case BCMA_CORE_NS_CHIPCOMMON_B:
+		case BCMA_CORE_PMU:
+		case BCMA_CORE_GCI:
 		/* Not used yet: case BCMA_CORE_OOB_ROUTER: */
 			break;
 		default:
--- a/drivers/net/wireless/b43/main.c
+++ b/drivers/net/wireless/b43/main.c
@@ -1215,10 +1215,10 @@ void b43_wireless_core_phy_pll_reset(str
 	case B43_BUS_BCMA:
 		bcma_cc = &dev->dev->bdev->bus->drv_cc;
 
-		bcma_cc_write32(bcma_cc, BCMA_CC_CHIPCTL_ADDR, 0);
-		bcma_cc_mask32(bcma_cc, BCMA_CC_CHIPCTL_DATA, ~0x4);
-		bcma_cc_set32(bcma_cc, BCMA_CC_CHIPCTL_DATA, 0x4);
-		bcma_cc_mask32(bcma_cc, BCMA_CC_CHIPCTL_DATA, ~0x4);
+		bcma_cc_write32(bcma_cc, BCMA_CC_PMU_CHIPCTL_ADDR, 0);
+		bcma_cc_mask32(bcma_cc, BCMA_CC_PMU_CHIPCTL_DATA, ~0x4);
+		bcma_cc_set32(bcma_cc, BCMA_CC_PMU_CHIPCTL_DATA, 0x4);
+		bcma_cc_mask32(bcma_cc, BCMA_CC_PMU_CHIPCTL_DATA, ~0x4);
 		break;
 #endif
 #ifdef CONFIG_B43_SSB
--- a/include/linux/bcma/bcma.h
+++ b/include/linux/bcma/bcma.h
@@ -151,6 +151,8 @@ struct bcma_host_ops {
 #define BCMA_CORE_PCIE2			0x83C	/* PCI Express Gen2 */
 #define BCMA_CORE_USB30_DEV		0x83D
 #define BCMA_CORE_ARM_CR4		0x83E
+#define BCMA_CORE_GCI			0x840
+#define BCMA_CORE_CMEM			0x846	/* CNDS DDR2/3 memory controller */
 #define BCMA_CORE_ARM_CA7		0x847
 #define BCMA_CORE_SYS_MEM		0x849
 #define BCMA_CORE_DEFAULT		0xFFF
@@ -200,6 +202,7 @@ struct bcma_host_ops {
 #define  BCMA_PKG_ID_BCM4707	1
 #define  BCMA_PKG_ID_BCM4708	2
 #define  BCMA_PKG_ID_BCM4709	0
+#define BCMA_CHIP_ID_BCM47094	53030
 #define BCMA_CHIP_ID_BCM53018	53018
 
 /* Board types (on PCI usually equals to the subsystem dev id) */
--- a/include/linux/bcma/bcma_driver_chipcommon.h
+++ b/include/linux/bcma/bcma_driver_chipcommon.h
@@ -217,6 +217,11 @@
 #define	 BCMA_CC_CLKDIV_JTAG_SHIFT	8
 #define	 BCMA_CC_CLKDIV_UART		0x000000FF
 #define BCMA_CC_CAP_EXT			0x00AC		/* Capabilities */
+#define  BCMA_CC_CAP_EXT_SECI_PRESENT	0x00000001
+#define  BCMA_CC_CAP_EXT_GSIO_PRESENT	0x00000002
+#define  BCMA_CC_CAP_EXT_GCI_PRESENT	0x00000004
+#define  BCMA_CC_CAP_EXT_SECI_PUART_PRESENT		0x00000008    /* UART present */
+#define  BCMA_CC_CAP_EXT_AOB_PRESENT	0x00000040
 #define BCMA_CC_PLLONDELAY		0x00B0		/* Rev >= 4 only */
 #define BCMA_CC_FREFSELDELAY		0x00B4		/* Rev >= 4 only */
 #define BCMA_CC_SLOWCLKCTL		0x00B8		/* 6 <= Rev <= 9 only */
@@ -351,12 +356,12 @@
 #define BCMA_CC_PMU_RES_REQTS		0x0640 /* PMU res req timer sel */
 #define BCMA_CC_PMU_RES_REQT		0x0644 /* PMU res req timer */
 #define BCMA_CC_PMU_RES_REQM		0x0648 /* PMU res req mask */
-#define BCMA_CC_CHIPCTL_ADDR		0x0650
-#define BCMA_CC_CHIPCTL_DATA		0x0654
-#define BCMA_CC_REGCTL_ADDR		0x0658
-#define BCMA_CC_REGCTL_DATA		0x065C
-#define BCMA_CC_PLLCTL_ADDR		0x0660
-#define BCMA_CC_PLLCTL_DATA		0x0664
+#define BCMA_CC_PMU_CHIPCTL_ADDR	0x0650
+#define BCMA_CC_PMU_CHIPCTL_DATA	0x0654
+#define BCMA_CC_PMU_REGCTL_ADDR		0x0658
+#define BCMA_CC_PMU_REGCTL_DATA		0x065C
+#define BCMA_CC_PMU_PLLCTL_ADDR		0x0660
+#define BCMA_CC_PMU_PLLCTL_DATA		0x0664
 #define BCMA_CC_PMU_STRAPOPT		0x0668 /* (corerev >= 28) */
 #define BCMA_CC_PMU_XTAL_FREQ		0x066C /* (pmurev >= 10) */
 #define  BCMA_CC_PMU_XTAL_FREQ_ILPCTL_MASK	0x00001FFF
@@ -566,6 +571,7 @@
  * Check availability with ((struct bcma_chipcommon)->capabilities & BCMA_CC_CAP_PMU)
  */
 struct bcma_chipcommon_pmu {
+	struct bcma_device *core;	/* Can be separated core or just ChipCommon one */
 	u8 rev;			/* PMU revision */
 	u32 crystalfreq;	/* The active crystal frequency (in kHz) */
 };
@@ -663,6 +669,19 @@ struct bcma_drv_cc_b {
 #define bcma_cc_maskset32(cc, offset, mask, set) \
 	bcma_cc_write32(cc, offset, (bcma_cc_read32(cc, offset) & (mask)) | (set))
 
+/* PMU registers access */
+#define bcma_pmu_read32(cc, offset) \
+	bcma_read32((cc)->pmu.core, offset)
+#define bcma_pmu_write32(cc, offset, val) \
+	bcma_write32((cc)->pmu.core, offset, val)
+
+#define bcma_pmu_mask32(cc, offset, mask) \
+	bcma_pmu_write32(cc, offset, bcma_pmu_read32(cc, offset) & (mask))
+#define bcma_pmu_set32(cc, offset, set) \
+	bcma_pmu_write32(cc, offset, bcma_pmu_read32(cc, offset) | (set))
+#define bcma_pmu_maskset32(cc, offset, mask, set) \
+	bcma_pmu_write32(cc, offset, (bcma_pmu_read32(cc, offset) & (mask)) | (set))
+
 extern u32 bcma_chipco_watchdog_timer_set(struct bcma_drv_cc *cc, u32 ticks);
 
 extern u32 bcma_chipco_get_alp_clock(struct bcma_drv_cc *cc);
--- a/drivers/bcma/bcma_private.h
+++ b/drivers/bcma/bcma_private.h
@@ -45,7 +45,6 @@ void bcma_core_chipcommon_early_init(str
 void bcma_core_chipcommon_init(struct bcma_drv_cc *cc);
 void bcma_chipco_bcm4331_ext_pa_lines_ctl(struct bcma_drv_cc *cc, bool enable);
 #ifdef CONFIG_BCMA_DRIVER_MIPS
-void bcma_chipco_serial_init(struct bcma_drv_cc *cc);
 extern struct platform_device bcma_pflash_dev;
 #endif /* CONFIG_BCMA_DRIVER_MIPS */
 
--- a/drivers/bcma/driver_gpio.c
+++ b/drivers/bcma/driver_gpio.c
@@ -229,6 +229,7 @@ int bcma_gpio_init(struct bcma_drv_cc *c
 	case BCMA_CHIP_ID_BCM4707:
 	case BCMA_CHIP_ID_BCM5357:
 	case BCMA_CHIP_ID_BCM53572:
+	case BCMA_CHIP_ID_BCM47094:
 		chip->ngpio	= 32;
 		break;
 	default:
--- a/drivers/bcma/driver_mips.c
+++ b/drivers/bcma/driver_mips.c
@@ -328,12 +328,9 @@ static void bcma_core_mips_flash_detect(
 
 void bcma_core_mips_early_init(struct bcma_drv_mips *mcore)
 {
-	struct bcma_bus *bus = mcore->core->bus;
-
 	if (mcore->early_setup_done)
 		return;
 
-	bcma_chipco_serial_init(&bus->drv_cc);
 	bcma_core_mips_flash_detect(mcore);
 
 	mcore->early_setup_done = true;
--- a/drivers/bcma/host_pci.c
+++ b/drivers/bcma/host_pci.c
@@ -294,7 +294,7 @@ static const struct pci_device_id bcma_p
 	{ PCI_DEVICE(PCI_VENDOR_ID_BROADCOM, 0x4358) },
 	{ PCI_DEVICE(PCI_VENDOR_ID_BROADCOM, 0x4359) },
 	{ PCI_DEVICE(PCI_VENDOR_ID_BROADCOM, 0x4360) },
-	{ PCI_DEVICE(PCI_VENDOR_ID_BROADCOM, 0x4365) },
+	{ PCI_DEVICE_SUB(PCI_VENDOR_ID_BROADCOM, 0x4365, PCI_VENDOR_ID_DELL, 0x0016) },
 	{ PCI_DEVICE(PCI_VENDOR_ID_BROADCOM, 0x43a0) },
 	{ PCI_DEVICE(PCI_VENDOR_ID_BROADCOM, 0x43a9) },
 	{ PCI_DEVICE(PCI_VENDOR_ID_BROADCOM, 0x43aa) },
