From 7f00ee2bbc630900ba16fc2690473f3e2db0e264 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <rafal@milecki.pl>
Date: Tue, 27 Sep 2016 14:11:04 +0200
Subject: [PATCH] brcmfmac: use correct skb freeing helper when deleting
 flowring
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Flowrings contain skbs waiting for transmission that were passed to us
by netif. It means we checked every one of them looking for 802.1x
Ethernet type. When deleting flowring we have to use freeing function
that will check for 802.1x type as well.

Freeing skbs without a proper check was leading to counter not being
properly decreased. This was triggering a WARNING every time
brcmf_netdev_wait_pend8021x was called.

Signed-off-by: RafaÅ MiÅecki <rafal@milecki.pl>
Acked-by: Arend van Spriel <arend@broadcom.com>
Cc: stable@vger.kernel.org # 4.5+
Signed-off-by: Kalle Valo <kvalo@codeaurora.org>
---
 drivers/net/wireless/broadcom/brcm80211/brcmfmac/flowring.c | 9 ++++++++-
 1 file changed, 8 insertions(+), 1 deletion(-)

--- a/drivers/net/wireless/broadcom/brcm80211/brcmfmac/flowring.c
+++ b/drivers/net/wireless/broadcom/brcm80211/brcmfmac/flowring.c
@@ -234,13 +234,20 @@ static void brcmf_flowring_block(struct
 
 void brcmf_flowring_delete(struct brcmf_flowring *flow, u16 flowid)
 {
+	struct brcmf_bus *bus_if = dev_get_drvdata(flow->dev);
 	struct brcmf_flowring_ring *ring;
+	struct brcmf_if *ifp;
 	u16 hash_idx;
+	u8 ifidx;
 	struct sk_buff *skb;
 
 	ring = flow->rings[flowid];
 	if (!ring)
 		return;
+
+	ifidx = brcmf_flowring_ifidx_get(flow, flowid);
+	ifp = brcmf_get_ifp(bus_if->drvr, ifidx);
+
 	brcmf_flowring_block(flow, flowid, false);
 	hash_idx = ring->hash_id;
 	flow->hash[hash_idx].ifidx = BRCMF_FLOWRING_INVALID_IFIDX;
@@ -249,7 +256,7 @@ void brcmf_flowring_delete(struct brcmf_
 
 	skb = skb_dequeue(&ring->skblist);
 	while (skb) {
-		brcmu_pkt_buf_free_skb(skb);
+		brcmf_txfinalize(ifp, skb, false);
 		skb = skb_dequeue(&ring->skblist);
 	}
 
