From 98e13e05a1bab82c3bec1d867159bc8384acbe5b Mon Sep 17 00:00:00 2001
From: Hauke Mehrtens <hauke@hauke-m.de>
Date: Thu, 11 Jun 2015 22:57:36 +0200
Subject: [PATCH] USB: bcma: replace numbers with constants

The constants for these numbers were added long time ago, use them.

Signed-off-by: Hauke Mehrtens <hauke@hauke-m.de>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 drivers/usb/host/bcma-hcd.c | 3 ++-
 1 file changed, 2 insertions(+), 1 deletion(-)

--- a/drivers/usb/host/bcma-hcd.c
+++ b/drivers/usb/host/bcma-hcd.c
@@ -233,7 +233,8 @@ static int bcma_hcd_probe(struct bcma_de
 
 	/* In AI chips EHCI is addrspace 0, OHCI is 1 */
 	ohci_addr = dev->addr_s[0];
-	if ((chipinfo->id == 0x5357 || chipinfo->id == 0x4749)
+	if ((chipinfo->id == BCMA_CHIP_ID_BCM5357 ||
+	     chipinfo->id == BCMA_CHIP_ID_BCM4749)
 	    && chipinfo->rev == 0)
 		ohci_addr = 0x18009000;
 
