From 672e48427ca17fadd59d294eec56476dd6a75398 Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.org>
Date: Fri, 23 Jan 2015 15:18:03 +0000
Subject: [PATCH 076/114] BCM2708_DT: Build the overlays as well

---
 arch/arm/boot/dts/Makefile | 13 +++++++++++++
 1 file changed, 13 insertions(+)

--- a/arch/arm/boot/dts/Makefile
+++ b/arch/arm/boot/dts/Makefile
@@ -55,6 +55,14 @@ dtb-$(CONFIG_ARCH_ATLAS6) += atlas6-evb.
 dtb-$(CONFIG_ARCH_AXXIA) += axm5516-amarillo.dtb
 dtb-$(CONFIG_BCM2708_DT) += bcm2708-rpi-b.dtb
 dtb-$(CONFIG_BCM2708_DT) += bcm2708-rpi-b-plus.dtb
+dtb-$(CONFIG_BCM2708_DT) += hifiberry-dac-overlay.dtb
+dtb-$(CONFIG_BCM2708_DT) += hifiberry-dacplus-overlay.dtb
+dtb-$(CONFIG_BCM2708_DT) += hifiberry-digi-overlay.dtb
+dtb-$(CONFIG_BCM2708_DT) += iqaudio-dac-overlay.dtb
+dtb-$(CONFIG_BCM2708_DT) += iqaudio-dacplus-overlay.dtb
+dtb-$(CONFIG_BCM2708_DT) += lirc-rpi-overlay.dtb
+dtb-$(CONFIG_BCM2708_DT) += w1-gpio-overlay.dtb
+dtb-$(CONFIG_BCM2708_DT) += w1-gpio-pullup-overlay.dtb
 dtb-$(CONFIG_ARCH_BCM2835) += bcm2835-rpi-b.dtb
 dtb-$(CONFIG_ARCH_BCM_5301X) += bcm4708-netgear-r6250.dtb
 dtb-$(CONFIG_ARCH_BCM_63XX) += bcm963138dvt.dtb
@@ -524,6 +532,11 @@ targets += $(dtb-y)
 
 endif
 
+# Enable fixups to support overlays on BCM2708 platforms
+ifeq ($(CONFIG_BCM2708_DT),y)
+	DTC_FLAGS ?= -@
+endif
+
 # *.dtb used to be generated in the directory above. Clean out the
 # old build results so people don't accidentally use them.
 dtbs: $(addprefix $(obj)/, $(dtb-y))
