From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <zajec5@gmail.com>
Date: Sun, 6 Dec 2015 10:21:00 +0100
Subject: [PATCH] ARM: BCM5301X: Fix fixed-clock frequency of some devices
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Some devices (mostly BCM4709 based) use higher clock.

Signed-off-by: Rafał Miłecki <zajec5@gmail.com>
---
 arch/arm/boot/dts/bcm4709-netgear-r8000.dts | 6 ++++++
 1 file changed, 6 insertions(+)

--- a/arch/arm/boot/dts/bcm4709-netgear-r8000.dts
+++ b/arch/arm/boot/dts/bcm4709-netgear-r8000.dts
@@ -25,6 +25,12 @@
 		       0x88000000 0x08000000>;
 	};
 
+	clocks {
+		clk_periph: periph {
+			clock-frequency = <500000000>;
+		};
+	};
+
 	leds {
 		compatible = "gpio-leds";
 
--- a/arch/arm/boot/dts/bcm47094-netgear-r8500.dts
+++ b/arch/arm/boot/dts/bcm47094-netgear-r8500.dts
@@ -25,6 +25,12 @@
 		       0x88000000 0x18000000>;
 	};
 
+	clocks {
+		clk_periph: periph {
+			clock-frequency = <700000000>;
+		};
+	};
+
 	leds {
 		compatible = "gpio-leds";
 
