From 2f0e56fa37cce60a5ac5d451bcadec51cd711436 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <rafal@milecki.pl>
Date: Tue, 27 Sep 2016 12:12:24 +0200
Subject: [PATCH] brcmfmac: replace WARNING on timeout with a simple error
 message
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Even with timeout increased to 950 ms we get WARNINGs from time to time.
It mostly happens on A-MPDU stalls (e.g. when station goes out of
range). It may take up to 5-10 secods for the firmware to recover and
for that time it doesn't process packets.

It's still useful to have a message on time out as it may indicate some
firmware problem and incorrect key update. Raising a WARNING however
wasn't really that necessary, it doesn't point to any driver bug anymore
and backtrace wasn't much useful.

Signed-off-by: RafaÅ MiÅecki <rafal@milecki.pl>
Acked-by: Arend van Spriel <arend.vanspriel@broadcom.com>
Signed-off-by: Kalle Valo <kvalo@codeaurora.org>
---
 drivers/net/wireless/broadcom/brcm80211/brcmfmac/core.c | 3 ++-
 1 file changed, 2 insertions(+), 1 deletion(-)

--- a/drivers/net/wireless/broadcom/brcm80211/brcmfmac/core.c
+++ b/drivers/net/wireless/broadcom/brcm80211/brcmfmac/core.c
@@ -1155,7 +1155,8 @@ int brcmf_netdev_wait_pend8021x(struct b
 				 !brcmf_get_pend_8021x_cnt(ifp),
 				 MAX_WAIT_FOR_8021X_TX);
 
-	WARN_ON(!err);
+	if (!err)
+		brcmf_err("Timed out waiting for no pending 802.1x packets\n");
 
 	return !err;
 }
