From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <zajec5@gmail.com>
Date: Sat, 18 Jun 2016 18:49:38 +0200
Subject: [PATCH] brcmfmac: include also core.h header in cfg80211.h
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

This header provides two inline functions using struct brcmf_if so we
need core.h to avoid:

drivers/net/wireless/broadcom/brcm80211/brcmfmac/cfg80211.h: In function ândev_to_profâ:
drivers/net/wireless/broadcom/brcm80211/brcmfmac/cfg80211.h:368:13: error: dereferencing pointer to incomplete type
  return &ifp->vif->profile;
             ^
drivers/net/wireless/broadcom/brcm80211/brcmfmac/cfg80211.h: In function ândev_to_vifâ:
drivers/net/wireless/broadcom/brcm80211/brcmfmac/cfg80211.h:374:12: error: dereferencing pointer to incomplete type
  return ifp->vif;
            ^

Signed-off-by: RafaÅ MiÅecki <zajec5@gmail.com>
Signed-off-by: Kalle Valo <kvalo@codeaurora.org>
---

--- a/drivers/net/wireless/broadcom/brcm80211/brcmfmac/cfg80211.h
+++ b/drivers/net/wireless/broadcom/brcm80211/brcmfmac/cfg80211.h
@@ -20,6 +20,7 @@
 /* for brcmu_d11inf */
 #include <brcmu_d11.h>
 
+#include "core.h"
 #include "fwil_types.h"
 #include "p2p.h"
 
