From 406d86e5990ac171f18ef6e2973672d8fbfe1556 Mon Sep 17 00:00:00 2001
From: Gabor Juhos <juhosg@openwrt.org>
Date: Wed, 20 Feb 2013 08:40:33 +0100
Subject: [PATCH] powerpc: 85xx: add support for the TP-Link TL-WDR4900 v1
 board

This patch adds support for the TP-Link TL-WDR4900 v1
concurrent dual-band wireless router. The devices uses
the Freescale P1014 SoC.

Signed-off-by: Gabor Juhos <juhosg@openwrt.org>
---
 arch/powerpc/boot/Makefile                  |   3 +
 arch/powerpc/boot/wrapper                   |   4 +
 arch/powerpc/platforms/85xx/Kconfig         |  11 ++
 arch/powerpc/platforms/85xx/Makefile        |   1 +

--- a/arch/powerpc/boot/Makefile
+++ b/arch/powerpc/boot/Makefile
@@ -112,6 +112,7 @@ src-plat-$(CONFIG_PPC_POWERNV) += pserie
 src-plat-$(CONFIG_PPC_IBM_CELL_BLADE) += pseries-head.S
 src-plat-$(CONFIG_PPC_CELLEB) += pseries-head.S
 src-plat-$(CONFIG_PPC_CELL_QPACE) += pseries-head.S
+src-plat-$(CONFIG_TL_WDR4900_V1) += cuboot-tl-wdr4900-v1.c
 
 src-wlib := $(sort $(src-wlib-y))
 src-plat := $(sort $(src-plat-y))
@@ -296,6 +297,7 @@ image-$(CONFIG_TQM8555)			+= cuImage.tqm
 image-$(CONFIG_TQM8560)			+= cuImage.tqm8560
 image-$(CONFIG_SBC8548)			+= cuImage.sbc8548
 image-$(CONFIG_KSI8560)			+= cuImage.ksi8560
+image-$(CONFIG_TL_WDR4900_V1)		+= cuImage.tl-wdr4900-v1
 
 # Board ports in arch/powerpc/platform/embedded6xx/Kconfig
 image-$(CONFIG_STORCENTER)		+= cuImage.storcenter
--- a/arch/powerpc/boot/wrapper
+++ b/arch/powerpc/boot/wrapper
@@ -218,6 +218,10 @@ cuboot*)
     *-mpc85*|*-tqm85*|*-sbc85*)
         platformo=$object/cuboot-85xx.o
         ;;
+    *-tl-wdr4900-v1)
+        platformo=$object/cuboot-tl-wdr4900-v1.o
+	link_address='0x1000000'
+        ;;
     *-amigaone)
         link_address='0x800000'
         ;;
--- a/arch/powerpc/platforms/85xx/Kconfig
+++ b/arch/powerpc/platforms/85xx/Kconfig
@@ -168,6 +168,17 @@ config STX_GP3
 	select CPM2
 	select DEFAULT_UIMAGE
 
+config TL_WDR4900_V1
+	bool "TP-Link TL-WDR4900 v1"
+	select DEFAULT_UIMAGE
+	select ARCH_REQUIRE_GPIOLIB
+	select GPIO_MPC8XXX
+	help
+	  This option enables support for the TP-Link TL-WDR4900 v1 board.
+
+	  This board is a Concurrent Dual-Band wireless router with a
+	  Freescale P1014 SoC.
+
 config TQM8540
 	bool "TQ Components TQM8540"
 	help
--- a/arch/powerpc/platforms/85xx/Makefile
+++ b/arch/powerpc/platforms/85xx/Makefile
@@ -23,6 +23,7 @@ obj-$(CONFIG_TWR_P102x)   += twr_p102x.o
 obj-$(CONFIG_CORENET_GENERIC)   += corenet_generic.o
 obj-$(CONFIG_STX_GP3)	  += stx_gp3.o
 obj-$(CONFIG_TQM85xx)	  += tqm85xx.o
+obj-$(CONFIG_TL_WDR4900_V1) += tl_wdr4900_v1.o
 obj-$(CONFIG_SBC8548)     += sbc8548.o
 obj-$(CONFIG_PPA8548)     += ppa8548.o
 obj-$(CONFIG_SOCRATES)    += socrates.o socrates_fpga_pic.o
